#
# various kinds of OPT RDATA stored in an input buffer
#
# empty RDATA (which is okay)
#
# 0  1 (bytes)
 00 00
#
# an OPT RR containing an NSID Option
#      code=3 len=3 ID value (opaque)
# 2  3  4  5  6  7  8  9 10
 00 07 00 03 00 03 00 01 02
#
# short buffer (this can be tested only at the end of the buffer)
# 1  2  3  4  5
 00 04 c0 00 02
