#   A response includes multiple DNAME and synchronized CNAME records
#   ;; ->>HEADER<<- opcode: QUERY, status: NOERROR, id: 900
#   ;; flags: qr aa rd; QUERY: 1, ANSWER: 4, AUTHORITY: 0, ADDITIONAL: 0
#   ;; WARNING: recursion requested but not available
#
#   ;; QUESTION SECTION:
#   ;a.dname.example.com.           IN      NS
#
#   ;; ANSWER SECTION:
#   dname.example.com.      21600   IN      DNAME   dname.example.org.
#   a.dname.example.com.    21600   IN      CNAME   a.dname.example.org.
#   dname.example.org.      21600   IN      DNAME   dname.example.org.
#   a.dname.example.org.    21600   IN      CNAME   a.dname.example.org.
0384 8500
 00 01 00 04 00 00 00 00 01 61 05 64
 6e 61 6d 65 07 65 78 61 6d 70 6c 65 03 63 6f 6d
 00 00 02 00 01 c0 0e 00 27 00 01 00 00 54 60 00
 13 05 64 6e 61 6d 65 07 65 78 61 6d 70 6c 65 03
 6f 72 67 00 c0 0c 00 05 00 01 00 00 54 60 00 04
 01 61 c0 31 c0 31 00 27 00 01 00 00 54 60 00 13
 05 64 6e 61 6d 65 07 65 78 61 6d 70 6c 65 03 6f
 72 67 00 c0 50 00 05 00 01 00 00 54 60 00 02 c0
 50
